CAPACITY:

MAXIMUM TONNAGE CAPACITY 120 TON

OVERALL LENGTH OF BED & RAM 120"

DISTANCE BETWEEN HOUSINGS 102"

THROAT DEPTH 15.9"

STROKE LENGTH 15.7"

OPEN HEIGHT 23.6"

APPROACH SPEED 307 IPM

BENDING SPEED 28 IPM

RETURN SPEED 271 IPM

MOTOR 24 HP

APPROXIMATE WEIGHT 21,000 LBS

EQUIPPED WITH:

CADMAN 8-AXIS CNC CONTROL

Y-1 & Y-2 PROGRAMMABLE RAM AXIS

V-AXIS ADJUSTABLE CROWNING BED

X1/R/Z1/Z2/X-PRIME 5-AXIS BACK GAUGE